\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*

!!!AUTHORIZED ACCESS ONLY!!!

\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*

User Access Verification

Password:

Password:

R2>rn

Translating "rn"

% Unknown command or computer name, or unable to find computer address

R2>en

Password:

R2#config t

Enter configuration commands, one per line. End with CNTL/Z.

R2(config)#no ip domain-lookup

R2(config)#enable secret class

R2(config)#banner motd &

Enter TEXT message. End with the character '&'.

\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*

!!!AUTHORIZED ACCESS ONLY!!!

\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*

&

R2(config)#line console 0

R2(config-line)#password cisco

R2(config-line)#login

R2(config-line)#exit

R2(config)#line vty 0 4

R2(config-line)#password cisco

R2(config-line)#login

R2(config-line)#exit

R2(config)#interface serial 0/0/0

R2(config-if)#ip address 192.168.2.2 255.255.255.0

R2(config-if)#no shutdown

R2(config-if)#interface fastethernet 0/0

R2(config-if)#ip address 192.168.3.1 255.255.255.0

R2(config-if)#no shutdown

R2(config-if)#end

R2#

%SYS-5-CONFIG\_I: Configured from console by console

R2#copy running-config startup-config

Destination filename [startup-config]?

Building configuration...

[OK]

R2#show ip route

Codes: C - connected, S - static, I - IGRP, R - RIP, M - mobile, B - BGP

D - EIGRP, EX - EIGRP external, O - OSPF, IA - OSPF inter area

N1 - OSPF NSSA external type 1, N2 - OSPF NSSA external type 2

E1 - OSPF external type 1, E2 - OSPF external type 2, E - EGP

i - IS-IS, L1 - IS-IS level-1, L2 - IS-IS level-2, ia - IS-IS inter area

\* - candidate default, U - per-user static route, o - ODR

P - periodic downloaded static route

Gateway of last resort is not set

C 192.168.2.0/24 is directly connected, Serial0/0/0

C 192.168.3.0/24 is directly connected, FastEthernet0/0

R2#show ip interface brief

Interface IP-Address OK? Method Status Protocol

FastEthernet0/0 192.168.3.1 YES manual up up

FastEthernet0/1 unassigned YES unset administratively down down

Serial0/0/0 192.168.2.2 YES manual up up

Serial0/0/1 unassigned YES unset administratively down down

Vlan1 unassigned YES unset administratively down down